SM-Table 2: Baseline fluid and poroelastic parameters.

|  |  |  |  |
| --- | --- | --- | --- |
| **Fluid and Poroelastic Parameters** | **Symbols** | **Values** | |
| M2 tidal angular frequency | (rad.s-1) | 1.40810-4 | |
| Density of seawater | (kg.m-3) | 1040.9/ 1043.9 / 1042.3 a | |
| Density of hydrothermal fluids | (kg.m-3) | 714.6 / 727.3/ 719.9 b | |
| Fluid viscosity | *μ* (Pa.s) | 10−5 c | |
|  |  | ***Layer 2A*** | ***Layer 2B/C*** |
| P wave velocity | *Vp* (m/s) | 2200d | 5500e |
| S wave velocity | *Vs* (m/s) | 431 | 2940 |
| Porosity | *ϕ* | 0.2f | 0.03g |
| Bulk density | (kg.m-3) | 2568.6 | 2892.8 |
| Grain bulk modulus | *Kg* (GPa) | 50h | 70i |
| Fluid bulk modulus | *Kf* (GPa) | 2.07j | 2.07j |
| Matrix (drained) bulk modulus | *Km* (GPa) | 4.2 | 49.4 |
| Storage compressibility for 1-D loading | *S1* (Pa-1) | 2.8210-10 | 1.9310-11 |

a Density of seawater for LSHF/EPR/MEF. Calculated for pressure at 200 bar and background seawater temperature at 4.4°C (LSHF); for pressure at 250 bar and background seawater temperature at 1.8°C (EPR) and for pressure at 220 bar and background seawater temperature at 2°C (MEF); from Holzbecher (1998); Rabinowicz et al. (1999); Fontaine et al. (2001).

b Density of hydrothermal fluids for LSHF/EPR/MEF. Calculated for pressure at 200 bar and hydrothermal fluid temperature at 330°C (LSHF); for pressure at 250 bar and hydrothermal fluid temperature at 330°C (EPR) and for pressure at 220 bar and hydrothermal fluid temperature at 330°C (MEF); from Holzbecher (1998); Rabinowicz et al. (1999); Fontaine et al. (2001).

c Calculated for hydrothermal fluid temperature at 330°C; from Fontaine et al. (2001).

d Sohn et al. (2004).

e Vera et al. (1990).

f Luyendyk (1984).

g Becker (1985).

h Carmichael (1966); Christensen and Salisbury (1972).

i Pros et al. (1962).

j Crone and Wilcock (2005), computed from the equations of state.

Becker, K. (1985), Large-scale electrical resistivity and bulk porosity of the oceanic crust, Deep Sea Drilling Project Hole 504B. Costa Rica Rift: Initial Rep. Deep Sea Drill. Proj. 83, 419–427. http://dx.doi.org/10.1029/1999JB900250.

Carmichael, R.S. (1966), Handbook of Physical Properties of Rocks, II. CRC Press, Boca Raton, FL. 345 pp.

Christensen, N.I., Salisbury, M.H., 1972. Sea floor spreading, progressive alteration of layer 2 basalts, and associated changes in seismic velocities, *Earth Planet. Sci. Lett.* 15, 367–375.

Crone, T.J., Wilcock, S.D. (2005), Modeling the effects of tidal loading on mid-ocean ridge hydrothermal systems, *Geochem. Geophys. Geosyst.* 6, Q07001. http:// dx.doi.org/10.1029/2004GC000905.

Fontaine, F.J., Rabinowicz, M., Boulègue, J. (2001), Permeability changes due to mineral diagenesis in fractured crust: implications for hydrothermal circulation at mid-ocean ridges, *Earth Planet. Sci. Lett.*, 184, 407–425.

Holzbecher, E.O. (1998), Modeling Density-Driven Flow in Porous Media, Springer, New York.

Luyendyk, B.P. (1984), On-bottom gravity profile across the East Pacific Rise crest at 21° north, *Geophysics* 49 (12), 2166–2177.

Pros, Z., Vanek, J., Klima, K. (1962), The velocity of elastic waves in diabase and greywacke under pressure up to 4 kilobars, *Stud. Geophys. Geod.* 6, 347–367.

Rabinowicz, M., Sempéré, J.C., Genthon, P. (1999), Thermal convection in a vertical permeable slot: implications for hydrothermal circulation along mid-ocean ridges, *J. Geophys. Res.*, 104, 29275–29292.

Sohn, R.A., Webb, S.C., Hildebrand, J.A. (2004), Fine-scale seismic structure of the shallow volcanic crust on the East Pacific Rise at 9°50’N, *J. Geophys. Res.*, 109, B12104. <http://dx.doi.org/10.1029/2004JB003152>.

Vera, E.E., Mutter, J.C., Buhl, P., Orcutt, J.A., Harding, A.J., Kappus, M.E., Detrick, R.S., Brocher, T.M. (1990), The structure of 0- to 0.2-m.y.-old oceanic crust at 9°N on the East Pacific Rise from expanded spread profiles, *J. Geophys. Res.* 95 (B10), 15529–15556.